vca overdrive = 5,33 v-->on/of switch-(3.3k R ->100k lin pot -> vca ctrl in or left side of  R126 

second hp Filter = ground  --> on/of switch (3,3K R (100k lin pot --> r107 

resonance increase = 5,33 v-->on/of switch -(470R - 100k lin pot --> env mod pot pin 2

devilfish like resonance= R104 parallel with a 4k7 R and 100k lin pot and a on/of switch

accent increase = R107 parallel with a jumper wire and a on/of switch

som sort of vcf/vco FM = R76 parallel with a jumper wire (not tested)

VCA overdrive,.pre vcf (
Tricky part! Only if you want the vco mute!

remove R80 replace it with a 330k R ( a on/of switch with 3 positions -( a 10k R with a 100k lin pot ( make te 330k R on the first positon and  the 10k R on the  3e  , connect them parallel 
positon 1 is the normal mode, position 2 is vco mute, postion 3 is the overdrive.)

if you select the 3e postion the current wil go with the lowest resistance

You also kan leave r80 in place and make it parallel with a 10k R and a 100k lin pot and  a on/of switch!

[image: image1.png]rlandr2are in parallel

itch

Sway,

10K

100k lin pot




