


Storing a Program





3 Hold Shift and press Perf Mode/Store.


The Display starts flashing and the original program location is


shown.


4 Select a new location where you want to store the program by


turning the Program Dial.


To quickly jump to another bank, hold Shift and turn the Program


Dial.


The program that occupies the location that you select will be


active on the keyboard, making it possible to verify that you do not


accidentally overwrite something you wanted to keep.


5 Hold Shift and press the Store a second time to confirm your


choice. Your edited program has now replaced the previous one in


the location you specified.


â€˘ To cancel the store procedure, press any buttons on the panel before


you press Store the second time.


â€˘ With Memory Protect set to Off, a double tap on Shift + Store will store a program in its original location.





Storing a Performance


To Store a combination of Slots that you have made, hold Shift and press Store once. Press Perf Mode to activate Performance Mode, 


turn the Program Dial to select a location (A, b xx) and confirm by holding Shift and pressing Store once more.








Copy and Paste settings


Settings from one Slot can be copied to a virtual clipboard and then


be pasted to another Slot. This can be useful if a program needs to be moved from the lower part (A and B) to the upper part (C and D) in a split configuration or if you want a program to be copied from one performance to another.





1 Make sure that the Slot you wish to copy is in focus.


2 Hold Copy and press on the source Slot button.


â€?cPâ€? and a letter that indicates which Slot you have copied will be shown in the Display.


3 You can now turn the Program Dial to select a destination performance.


4 Hold Shift + Paste, and press the Slot button where you want


your settings to be copied to. â€?Psâ€? and the destination Slot will be shown in the Display. The settings will be copied to the edit buffer of the performance, the dot to the right in the Display will be lit to indicate this.





The content of the virtual clipboard will remain until you copy another setting or parameter, or turn off the Nord Lead 4. This makes it possible to paste the same data to several destinations.





If you want to keep the new settings you have created by coping,


make sure to save the program or performance.





The same procedure can be used to copy individual parameters.


1 Hold Copy and turn a knob - the source to be copied. The parameters value will be displayed in the Display.


2 Press Paste (Shift + Copy), and turn another knob - the destination.


The setting from the source will now be copied to the


destination.





The Copy/Paste functionality can be used to copy Morphs from


one program to another, and to copy Impulse Morphs within one


program or to another.


